<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="xilinx_devices_V6">
<description>v1.05 Xilinx FPGAs</description>
<packages>
<package name="TQ144">
<description>&lt;b&gt;TQ144 TQG144&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LQFP-48">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="xilinx_devices_V6" package="TQ144" value="6SLX9TQG144"/>
<element name="U$1" library="SparkFun-DigitalIC" package="LQFP-48" value="FT2232D"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="P3"/>
<contactref element="U1" pad="P13"/>
<contactref element="U1" pad="P25"/>
<contactref element="U1" pad="P49"/>
<contactref element="U1" pad="P54"/>
<contactref element="U1" pad="P68"/>
<contactref element="U1" pad="P77"/>
<contactref element="U1" pad="P91"/>
<contactref element="U1" pad="P96"/>
<contactref element="U1" pad="P108"/>
<contactref element="U1" pad="P113"/>
<contactref element="U1" pad="P130"/>
<contactref element="U1" pad="P136"/>
<contactref element="U1" pad="P3"/>
<contactref element="U1" pad="P13"/>
<contactref element="U1" pad="P25"/>
<contactref element="U1" pad="P49"/>
<contactref element="U1" pad="P54"/>
<contactref element="U1" pad="P68"/>
<contactref element="U1" pad="P77"/>
<contactref element="U1" pad="P91"/>
<contactref element="U1" pad="P96"/>
<contactref element="U1" pad="P108"/>
<contactref element="U1" pad="P113"/>
<contactref element="U1" pad="P130"/>
<contactref element="U1" pad="P136"/>
</signal>
<signal name="GND1">
<contactref element="U$1" pad="18"/>
</signal>
<signal name="GND2">
<contactref element="U$1" pad="25"/>
</signal>
<signal name="GND3">
<contactref element="U$1" pad="34"/>
</signal>
<signal name="VCCIOA">
<contactref element="U$1" pad="14"/>
</signal>
<signal name="AGND">
<contactref element="U$1" pad="45"/>
</signal>
<signal name="VCC2">
<contactref element="U$1" pad="42"/>
</signal>
<signal name="VCC1">
<contactref element="U$1" pad="3"/>
</signal>
<signal name="VDD">
<contactref element="U1" pad="P103"/>
<contactref element="U1" pad="P86"/>
<contactref element="U1" pad="P76"/>
<contactref element="U1" pad="P135"/>
<contactref element="U1" pad="P125"/>
<contactref element="U1" pad="P122"/>
<contactref element="U1" pad="P31"/>
<contactref element="U1" pad="P18"/>
<contactref element="U1" pad="P4"/>
<contactref element="U1" pad="P63"/>
<contactref element="U1" pad="P42"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
