<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.5" x2="70" y2="-0.5" width="0" layer="20"/>
<wire x1="70" y1="-0.5" x2="70" y2="62.447896875" width="0" layer="20"/>
<wire x1="70" y1="62.447896875" x2="0" y2="62.447896875" width="0" layer="20"/>
<wire x1="0" y1="62.447896875" x2="0" y2="-0.5" width="0" layer="20"/>
</plain>
<libraries>
<library name="linear-technology-3">
<description>&lt;b&gt;Linear Technology Devices&lt;/b&gt;&lt;p&gt;
http://www.linear.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Modified by szczepan@stud.fh-hannover.de&lt;/author&gt;</description>
<packages>
<package name="TSOT23-6">
</package>
</packages>
</library>
<library name="jicamarca">
<description>&lt;h1&gt;Jicamarca Library&lt;/h1&gt;
&lt;p&gt;
&lt;i&gt;Creado por Jorge Ortiz, 2013.09.13&lt;/i&gt;
&lt;h2&gt;Descripción&lt;/h2&gt;
&lt;p&gt; Esta librería de Eagle 5.9 incluye los diferentes dispositivos que se usan en todos los proyectos en Jicamarca, a excepción de los que estan incluídos por defecto en las librerias de instalación de Eagle.
&lt;p&gt; Uso: &lt;/p&gt;
&lt;p&gt;Para añadir nuevos dispositivos, se puede abrir la librería en eagle y añadir los dispositivos, símbolo y/o paquetes correspondiente manualmente&lt;/p&gt;
&lt;p&gt;Para añadir nuevos dispositivos desde otras librerías&lt;/p&gt;
&lt;ol&gt;
&lt;li&gt;Bajarse la libraría correspondiente de Internet y abrirla en Eagle Control Panel&lt;/li&gt;
&lt;li&gt;File &gt; Export &gt; Script (Creará un script con todas las partes de la librería)&lt;/li&gt;
&lt;li&gt;Script &gt; lbrdump.ulp &gt; [Script Exportado en paso anterior] (Creará un script por cada parte)&lt;/li&gt;
&lt;li&gt;Añadir la librería, el export, y las partes a SVN&lt;/li&gt;
&lt;li&gt;Copiar solo las partes necesarias al directorio jocamarca_library/all_parts&lt;/li&gt;
&lt;li&gt;Nota que algunos devices incluyen sus propios símbolos y multiples paquetes, añadir esos también aun si no se usan.&lt;/li&gt;
&lt;li&gt;Desde Eagle Control Panal, abror la librería jicamarca.lbr&lt;/li&gt;
&lt;li&gt;Hacer Run &gt; Script &gt; [Paquetes por importar]&lt;/li&gt;
&lt;li&gt;Hacer Run &gt; Script &gt; [Símbolos por importar]&lt;/li&gt;
&lt;li&gt;Hacer Run &gt; Script &gt; [Devices por importar]&lt;/li&gt;
&lt;li&gt;Comprobar que los nuevos dispositivos estan en la librería&lt;/li&gt;
&lt;li&gt;Hacer Rename al device para ponerle un prefix adecuado (IC_, CONN_, RES_, etc..) y guardar los cambios&lt;/li&gt;
&lt;li&gt;Hacer un commit en SVN a la nueva versión actualizada de la librería&lt;/li&gt;
&lt;/ol&gt;
&lt;p&gt;
Scripts originales e instrucciones bajados de &lt;a href="http://dangerousprototypes.com/docs/Dangerous_Prototypes_Cadsoft_Eagle_parts_library#Library_helper_scripts"&gt;Dangerous Prototypes&lt;/a&gt;.</description>
<packages>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CAPSMT_62_C10">
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SOT-223">
</package>
<package name="HTSSOP-20">
</package>
<package name="M−FLAT">
</package>
<package name="SRR7045">
</package>
<package name="CSD17313Q2">
</package>
<package name="TPS54622RHLR">
</package>
<package name="SER1390-473MLB">
</package>
<package name="VLP8040T-6R8M">
</package>
<package name="TPS54618RTER">
</package>
<package name="DFN-12-LEAD">
</package>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
<package name="BCAP0150-P270-T07">
</package>
<package name="MMS7341">
</package>
<package name="MCL1GB">
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp">
<description>&lt;b&gt;AMP Connectors&lt;/b&gt;&lt;p&gt;
RJ45 Jack connectors&lt;br&gt;
 Based on the previous libraris:
 &lt;ul&gt;
 &lt;li&gt;amp.lbr
 &lt;li&gt;amp-j.lbr
 &lt;li&gt;amp-mta.lbr
 &lt;li&gt;amp-nlok.lbr
 &lt;li&gt;amp-sim.lbr
 &lt;li&gt;amp-micro-match.lbr
 &lt;/ul&gt;
 Sources :
 &lt;ul&gt;
 &lt;li&gt;Catalog 82066 Revised 11-95 
 &lt;li&gt;Product Guide 296785 Rev. 8-99
 &lt;li&gt;Product Guide CD-ROM 1999
 &lt;li&gt;www.amp.com
 &lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X3MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="BatteryBoard">
<packages>
<package name="SOIC08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="_hhn_attiny25_45_85">
<description>&lt;h3&gt;ATMEL ATtiny 25 / 45 /48&lt;/h3&gt;
&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Supplied Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; &amp;nbsp; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; &amp;nbsp; = SOIC 08 EIAJ 208mil&lt;br /&gt;
&lt;b&gt;SS&lt;/b&gt; = SOIC 08 JEDEC 150mil&lt;br /&gt;
&lt;b&gt;X&lt;/b&gt;&gt; &amp;nbsp; = TSSOP 08 4.4mm&lt;/p&gt;

&lt;p&gt;&lt;u&gt;&lt;b&gt;Revisions / Changelog&lt;/b&gt;&lt;/u&gt;&lt;br /&gt;
&amp;bull; &amp;nbsp;5.0.0 [EAGLE 5]&lt;br /&gt;
&lt;/p&gt;

&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<packages>
<package name="SOIC8_EIAJ_208MIL">
<description>&lt;B&gt;Small Outline Medium Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
208-mil body</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="linear-technology-3" package="TSOT23-6" value="LTC4412ES6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="LTC4412ES6#TRPBF"/>
<attribute name="DIGIKEY#" value="LTC4412ES6#TRPBFCT-ND "/>
<attribute name="MANF" value="Linear Technology"/>
</element>
<element name="U6" library="jicamarca" package="SOT-223" value="SPX3940AM3-L-5-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="SPX3940AM3-L-5-0"/>
<attribute name="DIGIKEY#" value="1016-1558-5-ND"/>
<attribute name="MANF" value="Exar Corporation"/>
</element>
<element name="U3" library="jicamarca" package="HTSSOP-20" value="LM25118">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MOUSER#" value="926-LM25118MHE/NOPB"/>
<attribute name="MANF#" value="LM25118MHE/NOPB"/>
<attribute name="MANF" value="Texas Instruments"/>
</element>
<element name="CBOOT" library="jicamarca" package="C0805" value="0.1u">
<attribute name="DIGIKEY#" value="311-1140-1-ND"/>
<attribute name="VALUE" value="0.1u"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805KRX7R9BB104"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="CCOMP" library="jicamarca" package="C0805" value="180p">
<attribute name="DIGIKEY#" value="311-1114-1-ND"/>
<attribute name="VALUE" value="180p"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805JRNPO9BN181"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="CCOMP1" library="jicamarca" package="C0805" value="1.5n">
<attribute name="DIGIKEY#" value="311-1128-1-ND"/>
<attribute name="VALUE" value="1500p"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805KRX7R9BB152"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="CIN" library="jicamarca" package="C0805" value="4.7u">
<attribute name="DIGIKEY#" value="490-5422-1-ND"/>
<attribute name="VALUE" value="4.7u"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="GRM21BR61E475MA12L"/>
<attribute name="MANF" value="Murata"/>
</element>
<element name="CINX" library="jicamarca" package="C0805" value="0.1u">
<attribute name="DIGIKEY#" value="478-3755-1-ND"/>
<attribute name="VALUE" value="100n"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="08053C104KAT2A"/>
<attribute name="MANF" value="AVX"/>
</element>
<element name="COUT" library="jicamarca" package="C0805" value="4.7u">
<attribute name="DIGIKEY#" value="490-5422-1-ND"/>
<attribute name="VALUE" value="4.7u"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="GRM21BR61E475MA12L"/>
<attribute name="MANF" value="Murata"/>
</element>
<element name="CRAMP" library="jicamarca" package="C0805" value="680p">
<attribute name="DIGIKEY#" value="311-1126-1-ND"/>
<attribute name="VALUE" value="680p"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805KRX7R9BB681"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="CSS" library="jicamarca" package="C0805" value="470p">
<attribute name="DIGIKEY#" value="311-1124-1-ND"/>
<attribute name="VALUE" value="470p"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805KRX7R9BB471"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="CVCC" library="jicamarca" package="C0805" value="1u">
<attribute name="DIGIKEY#" value="587-1283-1-ND"/>
<attribute name="VALUE" value="1.0u"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="EMK212B7105KG-T"/>
<attribute name="MANF" value="Taiyo Yuden"/>
</element>
<element name="D1" library="jicamarca" package="M−FLAT" value="0.32v">
<attribute name="DIGIKEY#" value="CMS06QMCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CMS06(TE12L,Q,M)"/>
<attribute name="MANF" value="TOSHIBA"/>
</element>
<element name="D2" library="jicamarca" package="M−FLAT" value="0.32v">
<attribute name="DIGIKEY#" value="CMS06QMCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CMS06(TE12L,Q,M)"/>
<attribute name="MANF" value="TOSHIBA"/>
</element>
<element name="D3" library="jicamarca" package="M−FLAT" value="0.32v">
<attribute name="DIGIKEY#" value="CMS06QMCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CMS06(TE12L,Q,M)"/>
<attribute name="MANF" value="TOSHIBA"/>
</element>
<element name="D4" library="jicamarca" package="M−FLAT" value="0.32v">
<attribute name="DIGIKEY#" value="CMS06QMCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CMS06(TE12L,Q,M)"/>
<attribute name="MANF" value="TOSHIBA"/>
</element>
<element name="L1_2" library="jicamarca" package="SRR7045" value="1m">
<attribute name="DIGIKEY#S" value="1m:SRR7045-102M:SRR7045-102MCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Bourns Inc."/>
</element>
<element name="M2" library="jicamarca" package="CSD17313Q2" value="">
<attribute name="DIGIKEY#" value="296-27233-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CSD17313Q2"/>
<attribute name="MANF" value="Texas Instruments"/>
</element>
<element name="M1" library="jicamarca" package="CSD17313Q2" value="">
<attribute name="DIGIKEY#" value="296-27233-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CSD17313Q2"/>
<attribute name="MANF" value="Texas Instruments"/>
</element>
<element name="RCOMP" library="jicamarca" package="R0805" value="64.9K">
<attribute name="DIGIKEY#" value="P64.9KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF6492V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RENB_1" library="jicamarca" package="R0805" value="1000K">
<attribute name="DIGIKEY#" value="P1.00MCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="1000k"/>
<attribute name="MANF#" value="ERJ-6ENF1004V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RFBB" library="jicamarca" package="R0603" value="1k">
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="NAME"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
</element>
<element name="RFBT" library="jicamarca" package="R0402" value="8.66K">
<attribute name="DIGIKEY#" value="541-8.66KLCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CRCW04028K66FKED"/>
<attribute name="MANF" value="Vishay-Dale"/>
</element>
<element name="RSENSE" library="jicamarca" package="R0805" value="0.82">
<attribute name="DIGIKEY#" value="P.82DCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6RQFR82V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RT" library="jicamarca" package="R0805" value="61.9K">
<attribute name="DIGIKEY#" value="P61.9KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF6192V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RUV1" library="jicamarca" package="R0805" value="16.5k">
<attribute name="DIGIKEY#" value="P16.5KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF1652V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RUV2" library="jicamarca" package="R0805" value="3.4K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF3401V"/>
<attribute name="DIGIKEY#" value="P3.40KCCT-ND"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="U2" library="jicamarca" package="TPS54622RHLR" value="TPS54622">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="TPS54622RHLT"/>
<attribute name="DIGIKEY#" value="296-32493-1-ND"/>
<attribute name="MANF" value="Texas Instruments"/>
</element>
<element name="CCOMP_1" library="jicamarca" package="C0805" value="470n">
<attribute name="DIGIKEY#" value="587-1282-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="EMK212B7474KD-T"/>
<attribute name="MANF" value="Taiyo Yuden"/>
</element>
<element name="CBOOT_1" library="jicamarca" package="C0805" value="100n">
<attribute name="DIGIKEY#" value="478-3755-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="08053C104KAT2A"/>
<attribute name="MANF" value="AVX"/>
</element>
<element name="CCOMP2_1" library="jicamarca" package="C0805" value="1n">
<attribute name="DIGIKEY#" value="311-1127-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805KRX7R9BB102"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="CIN_1" library="jicamarca" package="C1210" value="22u">
<attribute name="DIGIKEY#" value="490-3889-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="GRM32ER61E226KE15L"/>
<attribute name="MANF" value="Murata"/>
</element>
<element name="CINX_1" library="jicamarca" package="C0805" value="4.7u">
<attribute name="DIGIKEY#" value="490-6467-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="4.7u"/>
<attribute name="MANF#" value="GRM21BC81E475KA12L"/>
<attribute name="MANF" value="Murata"/>
</element>
<element name="COUT_1" library="jicamarca" package="CAPSMT_62_C10" value="180u">
<attribute name="DIGIKEY#" value="P16476CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="16SVPE180M"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="CSS_1" library="jicamarca" package="C0805" value="150p">
<attribute name="DIGIKEY#" value="311-1113-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805JRNPO9BN151"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="L1_1" library="jicamarca" package="SER1390-473MLB" value="47u">
<attribute name="MOUSER#" value="994-SER1390-473MLB"/>
<attribute name="DCR" value="21m"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="SER1390-473MLB"/>
<attribute name="MANF" value="Coilcraft"/>
</element>
<element name="RCOMP_1" library="jicamarca" package="R0805" value="3.24k">
<attribute name="DIGIKEY#" value="P3.24KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF3241V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RENB_2" library="jicamarca" package="R0805" value="37.4k">
<attribute name="DIGIKEY#" value="P37.4KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF3742V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RENT_1" library="jicamarca" package="R0805" value="105k">
<attribute name="DIGIKEY#" value="P105KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF1053V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RFBB_1" library="jicamarca" package="R0805" value="10K">
<attribute name="DIGIKEY#" value="P10.0KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF1002V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RFBT_1" library="jicamarca" package="R0805" value="80.6k">
<attribute name="DIGIKEY#" value="P80.6KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF8062V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RT_1" library="jicamarca" package="R0805" value="243K">
<attribute name="DIGIKEY#" value="P243KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF2433V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="CBOOT_2" library="jicamarca" package="C0805" value="100n">
<attribute name="DIGIKEY#" value="478-3755-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="08053C104KAT2A"/>
<attribute name="MANF" value="AVX"/>
</element>
<element name="CCOMP2_2" library="jicamarca" package="C0805" value="150p">
<attribute name="DIGIKEY#" value="311-1113-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="CC0805JRNPO9BN151"/>
<attribute name="MANF" value="Yageo America"/>
</element>
<element name="CINX_2" library="jicamarca" package="C0805" value="100n">
<attribute name="DIGIKEY#" value="478-3755-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="08053C104KAT2A"/>
<attribute name="MANF" value="AVX"/>
</element>
<element name="RFBB_2" library="jicamarca" package="R0805" value="10K">
<attribute name="DIGIKEY#" value="P10.0KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF1002V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="CCOMP_2" library="jicamarca" package="C0805" value="47n">
<attribute name="DIGIKEY#" value="587-1280-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="TMK212B7473KD-T"/>
<attribute name="MANF" value="Taiyo Yuden"/>
</element>
<element name="CIN_2" library="jicamarca" package="C0805" value="10u">
<attribute name="DIGIKEY#" value="399-4925-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="10u"/>
<attribute name="MANF#" value="C0805C106K8PACTU"/>
<attribute name="MANF" value="Kemet"/>
</element>
<element name="COUT_2" library="jicamarca" package="C0805" value="22u">
<attribute name="DIGIKEY#" value="490-1719-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="22u"/>
<attribute name="MANF#" value="GRM21BR60J226ME39L"/>
<attribute name="MANF" value="Murata"/>
</element>
<element name="CSS_2" library="jicamarca" package="C0805" value="2.7n">
<attribute name="DIGIKEY#" value="GRM216R71E272KA01D-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="GRM216R71E272KA01D"/>
<attribute name="MANF" value="Murata"/>
</element>
<element name="L1_3" library="jicamarca" package="VLP8040T-6R8M" value="6.8u">
<attribute name="DIGIKEY#" value="445-6586-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="VLP8040T-6R8M"/>
<attribute name="MANF" value="TDK"/>
</element>
<element name="RCOMP_2" library="jicamarca" package="R0805" value="4.12k">
<attribute name="DIGIKEY#" value="P4.12KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF4121V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RENB_3" library="jicamarca" package="R0805" value="82.5k">
<attribute name="DIGIKEY#" value="P82.5KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF8252V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RENT_2" library="jicamarca" package="R0805" value="107k">
<attribute name="DIGIKEY#" value="P107KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF1073V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RFBT_2" library="jicamarca" package="R0805" value="31.6k">
<attribute name="DIGIKEY#" value="P31.6KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF3162V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RPG_1" library="jicamarca" package="R0805" value="49.9k">
<attribute name="DIGIKEY#" value="P49.9KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF4992V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="RT_2" library="jicamarca" package="R0805" value="432k">
<attribute name="DIGIKEY#" value="P432KCCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="ERJ-6ENF4323V"/>
<attribute name="MANF" value="Panasonic"/>
</element>
<element name="U7" library="jicamarca" package="TPS54618RTER" value="TPS54618RTER">
<attribute name="DIGIKEY#" value="296-28148-1-ND"/>
<attribute name="MANF#" value="TPS54618RTER"/>
<attribute name="MANF" value="Texas Instruments"/>
</element>
<element name="U5" library="jicamarca" package="DFN-12-LEAD" value="LTC3625">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="LTC3625EDE#PBF"/>
<attribute name="DIGIKEY#" value="LTC3625EDE#PBF-ND"/>
<attribute name="MANF" value="Linear Technology"/>
</element>
<element name="R5" library="jicamarca" package="R0805" value="294k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="78.7k:MCR10ERTF7872:RHM78.7KCHCT-ND|100k:MCR10ERTF1003:RHM100KCHCT-ND|294k:MCR10ERTF2943:RHM294KCHCT-ND|470k:MCR10ERTF4703:RHM470KCHCT-ND|10:TRR10EZPF10R0:RHM10.0BLCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="R6" library="jicamarca" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="78.7k:MCR10ERTF7872:RHM78.7KCHCT-ND|100k:MCR10ERTF1003:RHM100KCHCT-ND|294k:MCR10ERTF2943:RHM294KCHCT-ND|470k:MCR10ERTF4703:RHM470KCHCT-ND|10:TRR10EZPF10R0:RHM10.0BLCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="R8" library="jicamarca" package="R0805" value="78.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="78.7k:MCR10ERTF7872:RHM78.7KCHCT-ND|100k:MCR10ERTF1003:RHM100KCHCT-ND|294k:MCR10ERTF2943:RHM294KCHCT-ND|470k:MCR10ERTF4703:RHM470KCHCT-ND|10:TRR10EZPF10R0:RHM10.0BLCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="Q1" library="jicamarca" package="SOIC8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="SI4421DY-T1-E3"/>
<attribute name="DIGIKEY#" value="SI4421DY-T1-E3CT-ND"/>
<attribute name="MANF" value="Vishay Siliconix"/>
</element>
<element name="Q2" library="jicamarca" package="SOIC8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="SI4421DY-T1-E3"/>
<attribute name="DIGIKEY#" value="SI4421DY-T1-E3CT-ND"/>
<attribute name="MANF" value="Vishay Siliconix"/>
</element>
<element name="R9" library="jicamarca" package="R0805" value="470k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="78.7k:MCR10ERTF7872:RHM78.7KCHCT-ND|100k:MCR10ERTF1003:RHM100KCHCT-ND|294k:MCR10ERTF2943:RHM294KCHCT-ND|470k:MCR10ERTF4703:RHM470KCHCT-ND|10:TRR10EZPF10R0:RHM10.0BLCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="SC1" library="jicamarca" package="BCAP0150-P270-T07" value="150F">
<attribute name="DIGIKEY#" value="1182-1014-ND"/>
<attribute name="VMAX" value="2.7V"/>
<attribute name="MANF#" value="BCAP0150 P270 T07"/>
<attribute name="MANF" value="MAXWELL"/>
</element>
<element name="SC2" library="jicamarca" package="BCAP0150-P270-T07" value="150F">
<attribute name="DIGIKEY#" value="1182-1014-ND"/>
<attribute name="VMAX" value="2.7V"/>
<attribute name="MANF#" value="BCAP0150 P270 T07"/>
<attribute name="MANF" value="MAXWELL"/>
</element>
<element name="C1" library="jicamarca" package="C0805" value="10u">
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|10u:CL21A106KPCLQNC:1276-2402-1-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jicamarca" package="MCL1GB" value="6.8u">
<attribute name="DIGIKEY#" value="493-9749-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="UWG1E6R8MCL1GB"/>
<attribute name="MANF" value="Nichicon"/>
</element>
<element name="C3" library="jicamarca" package="MCL1GB" value="10u">
<attribute name="DIGIKEY#" value="493-9741-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF#" value="UWG1C100MCL1GB"/>
<attribute name="MANF" value="Nichicon"/>
</element>
<element name="R11" library="jicamarca" package="R0603" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="R7" library="jicamarca" package="R0603" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="R10" library="jicamarca" package="R0603" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="PWR_IN" library="con-amp" package="1X3MTA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jicamarca" package="R0603" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="PWR_OUT" library="con-lstb" package="MA04-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="JST-2-SMD" value="M02-JST-2MM-SMT">
<attribute name="PROD_ID" value="CONN-08352"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="jicamarca" package="MMS7341" value="3.3u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MOUSER#" value="994-MSS7341-332NLD"/>
<attribute name="MANF#" value="MSS7341-332NLD"/>
<attribute name="MANF" value="Coilcraft"/>
</element>
<element name="L2" library="jicamarca" package="MMS7341" value="3.3u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MOUSER#" value="994-MSS7341-332NLD"/>
<attribute name="MANF#" value="MSS7341-332NLD"/>
<attribute name="MANF" value="Coilcraft"/>
</element>
<element name="U1" library="BatteryBoard" package="SOIC08" value="DS2438Z">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="DIGIKEY#" value="DS2438Z+T&amp;RCT-ND"/>
<attribute name="MANF" value="Maxim Integrated"/>
<attribute name="MANF#" value="DS2438Z+T&amp;R"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PRG_6NS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jicamarca" package="R0805" value="402k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="P402KHCT-ND"/>
<attribute name="MANF" value="Panasonic"/>
<attribute name="MANF#" value="ERJ-3EKF4023V"/>
<attribute name="DIGIKEY#S" value="78.7k:MCR10ERTF7872:RHM78.7KCHCT-ND|100k:MCR10ERTF1003:RHM100KCHCT-ND|294k:MCR10ERTF2943:RHM294KCHCT-ND|470k:MCR10ERTF4703:RHM470KCHCT-ND|10:TRR10EZPF10R0:RHM10.0BLCT-ND"/>
</element>
<element name="R2" library="jicamarca" package="R0805" value="140k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="311-140KCRCT-ND"/>
<attribute name="MANF" value="Yageo"/>
<attribute name="MANF#" value="RC0805FR-07140KL"/>
<attribute name="DIGIKEY#S" value="78.7k:MCR10ERTF7872:RHM78.7KCHCT-ND|100k:MCR10ERTF1003:RHM100KCHCT-ND|294k:MCR10ERTF2943:RHM294KCHCT-ND|470k:MCR10ERTF4703:RHM470KCHCT-ND|10:TRR10EZPF10R0:RHM10.0BLCT-ND"/>
</element>
<element name="R4" library="jicamarca" package="R0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="311-4.70KCRCT-ND"/>
<attribute name="MANF" value="Yageo"/>
<attribute name="MANF#" value="RC0805FR-074K7L"/>
<attribute name="DIGIKEY#S" value="78.7k:MCR10ERTF7872:RHM78.7KCHCT-ND|100k:MCR10ERTF1003:RHM100KCHCT-ND|294k:MCR10ERTF2943:RHM294KCHCT-ND|470k:MCR10ERTF4703:RHM470KCHCT-ND|10:TRR10EZPF10R0:RHM10.0BLCT-ND"/>
</element>
<element name="U4" library="_hhn_attiny25_45_85" package="SOIC8_EIAJ_208MIL" value="ATTINY85-S">
<attribute name="MANF#" value="ATTINY85-15ST"/>
<attribute name="DIGIKEY#" value="ATTINY85-15STCT-ND"/>
<attribute name="MANF" value="Atmel"/>
</element>
<element name="R12" library="jicamarca" package="R0603" value="0">
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="R13" library="jicamarca" package="R0603" value="0">
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="R14" library="jicamarca" package="R0603" value="0">
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
<element name="R15" library="jicamarca" package="R0603" value="0">
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
</element>
</elements>
<signals>
<signal name="0V">
<contactref element="U5" pad="13"/>
<contactref element="R6" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="SC2" pad="-"/>
<contactref element="IC1" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="RUV1" pad="1"/>
<contactref element="RUV2" pad="2"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="RCOMP" pad="1"/>
<contactref element="CCOMP1" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U3" pad="9"/>
<contactref element="RCOMP" pad="2"/>
<contactref element="CCOMP" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U3" pad="8"/>
<contactref element="CCOMP1" pad="2"/>
<contactref element="RFBB" pad="2"/>
<contactref element="RFBT" pad="1"/>
<contactref element="CCOMP" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="U3" pad="7"/>
<contactref element="CSS" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U3" pad="5"/>
<contactref element="CRAMP" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="U3" pad="4"/>
<contactref element="RENB_1" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U3" pad="3"/>
<contactref element="RT" pad="2"/>
</signal>
<signal name="VIN_1">
<contactref element="RUV1" pad="2"/>
<contactref element="RENB_1" pad="2"/>
<contactref element="CIN" pad="1"/>
<contactref element="CINX" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="M1" pad="2"/>
<contactref element="M1" pad="8"/>
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="6"/>
<contactref element="M1" pad="5"/>
<contactref element="PWR_IN" pad="3"/>
</signal>
<signal name="VOUT_12">
<contactref element="U3" pad="10"/>
<contactref element="RFBT" pad="2"/>
<contactref element="D4" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="COUT" pad="1"/>
<contactref element="PWR_OUT" pad="2"/>
</signal>
<signal name="GND_12">
<contactref element="U3" pad="GND"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="14"/>
<contactref element="COUT" pad="2"/>
<contactref element="M2" pad="4"/>
<contactref element="M2" pad="7"/>
<contactref element="RSENSE" pad="1"/>
<contactref element="CVCC" pad="2"/>
<contactref element="U3" pad="13"/>
<contactref element="U3" pad="17"/>
<contactref element="RFBB" pad="1"/>
<contactref element="RUV2" pad="1"/>
<contactref element="RT" pad="1"/>
<contactref element="CRAMP" pad="2"/>
<contactref element="CSS" pad="2"/>
<contactref element="CINX" pad="2"/>
<contactref element="CIN" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="U3" pad="16"/>
<contactref element="CVCC" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="U3" pad="12"/>
<contactref element="D1" pad="2"/>
<contactref element="RSENSE" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="U3" pad="15"/>
<contactref element="M2" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="U3" pad="18"/>
<contactref element="CBOOT" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="D1" pad="1"/>
<contactref element="M1" pad="4"/>
<contactref element="M1" pad="7"/>
<contactref element="CBOOT" pad="2"/>
<contactref element="D2" pad="1"/>
<contactref element="L1_2" pad="1"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="N$43">
<contactref element="U3" pad="19"/>
<contactref element="M1" pad="3"/>
</signal>
<signal name="N$46">
<contactref element="L1_2" pad="2"/>
<contactref element="M2" pad="2"/>
<contactref element="M2" pad="8"/>
<contactref element="M2" pad="1"/>
<contactref element="M2" pad="6"/>
<contactref element="M2" pad="5"/>
<contactref element="D4" pad="2"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="VIN_2">
<contactref element="CIN_1" pad="1"/>
<contactref element="CINX_1" pad="1"/>
<contactref element="RENT_1" pad="2"/>
<contactref element="U2" pad="6"/>
<contactref element="PWR_IN" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="RENT_1" pad="1"/>
<contactref element="RENB_2" pad="2"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="N$44">
<contactref element="U2" pad="1"/>
<contactref element="RT_1" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="U2" pad="9"/>
<contactref element="CSS_1" pad="1"/>
</signal>
<signal name="GND_5">
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="2"/>
<contactref element="CSS_1" pad="2"/>
<contactref element="RT_1" pad="1"/>
<contactref element="RENB_2" pad="1"/>
<contactref element="CINX_1" pad="2"/>
<contactref element="CIN_1" pad="2"/>
<contactref element="CCOMP_1" pad="2"/>
<contactref element="CCOMP2_1" pad="2"/>
<contactref element="RFBB_1" pad="1"/>
<contactref element="L1_1" pad="3"/>
<contactref element="COUT_1" pad="C"/>
<contactref element="R7" pad="1"/>
<contactref element="PWR_IN" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="U2" pad="8"/>
<contactref element="RCOMP_1" pad="2"/>
<contactref element="CCOMP2_1" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="RCOMP_1" pad="1"/>
<contactref element="CCOMP_1" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="U2" pad="13"/>
<contactref element="CBOOT_1" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="U2" pad="12"/>
<contactref element="U2" pad="11"/>
<contactref element="CBOOT_1" pad="2"/>
<contactref element="L1_1" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="U2" pad="7"/>
<contactref element="RFBT_1" pad="1"/>
<contactref element="RFBB_1" pad="2"/>
</signal>
<signal name="VOUT_2">
<contactref element="RFBT_1" pad="2"/>
<contactref element="COUT_1" pad="A"/>
<contactref element="L1_1" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U5" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="5"/>
<contactref element="Q1" pad="7"/>
<contactref element="Q1" pad="8"/>
<contactref element="Q1" pad="6"/>
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="N$54">
<contactref element="RPG_1" pad="2"/>
<contactref element="U7" pad="14"/>
</signal>
<signal name="N$56">
<contactref element="RENT_2" pad="1"/>
<contactref element="RENB_3" pad="2"/>
<contactref element="U7" pad="15"/>
</signal>
<signal name="N$58">
<contactref element="RT_2" pad="2"/>
<contactref element="U7" pad="8"/>
</signal>
<signal name="N$59">
<contactref element="CSS_2" pad="1"/>
<contactref element="U7" pad="9"/>
</signal>
<signal name="GND_3">
<contactref element="CSS_2" pad="2"/>
<contactref element="RT_2" pad="1"/>
<contactref element="RENB_3" pad="1"/>
<contactref element="CINX_2" pad="1"/>
<contactref element="CIN_2" pad="2"/>
<contactref element="CCOMP2_2" pad="2"/>
<contactref element="CCOMP_2" pad="2"/>
<contactref element="RFBB_2" pad="1"/>
<contactref element="COUT_2" pad="2"/>
<contactref element="U7" pad="17"/>
<contactref element="U7" pad="5"/>
<contactref element="U7" pad="3"/>
<contactref element="U7" pad="4"/>
<contactref element="R11" pad="2"/>
<contactref element="PWR_OUT" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="RCOMP_2" pad="2"/>
<contactref element="CCOMP2_2" pad="1"/>
<contactref element="U7" pad="7"/>
</signal>
<signal name="N$63">
<contactref element="RCOMP_2" pad="1"/>
<contactref element="CCOMP_2" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="CBOOT_2" pad="1"/>
<contactref element="U7" pad="13"/>
</signal>
<signal name="N$66">
<contactref element="L1_3" pad="1"/>
<contactref element="CBOOT_2" pad="2"/>
<contactref element="U7" pad="12"/>
<contactref element="U7" pad="11"/>
<contactref element="U7" pad="10"/>
</signal>
<signal name="N$67">
<contactref element="RFBT_2" pad="1"/>
<contactref element="RFBB_2" pad="2"/>
<contactref element="U7" pad="6"/>
</signal>
<signal name="VIN_3">
<contactref element="RPG_1" pad="1"/>
<contactref element="RENT_2" pad="2"/>
<contactref element="CINX_2" pad="2"/>
<contactref element="CIN_2" pad="1"/>
<contactref element="U7" pad="1"/>
<contactref element="U7" pad="2"/>
<contactref element="U7" pad="16"/>
<contactref element="U6" pad="1"/>
<contactref element="C2" pad="P"/>
<contactref element="IC1" pad="6"/>
<contactref element="R9" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$16">
</signal>
<signal name="N$21">
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="QW">
<contactref element="R8" pad="2"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="N$57">
<contactref element="U5" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="U5" pad="12"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="U5" pad="10"/>
<contactref element="SC2" pad="+"/>
<contactref element="SC1" pad="-"/>
<contactref element="L1" pad="2"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$64">
<contactref element="U5" pad="11"/>
<contactref element="SC1" pad="+"/>
<contactref element="IC1" pad="1"/>
<contactref element="Q2" pad="5"/>
<contactref element="Q2" pad="7"/>
<contactref element="Q2" pad="8"/>
<contactref element="Q2" pad="6"/>
</signal>
<signal name="N$68">
<contactref element="IC1" pad="5"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$69">
<contactref element="IC1" pad="4"/>
<contactref element="R9" pad="1"/>
<contactref element="Q1" pad="4"/>
</signal>
<signal name="N$47">
<contactref element="IC1" pad="3"/>
<contactref element="U5" pad="8"/>
</signal>
<signal name="VOUT_5">
<contactref element="U6" pad="3"/>
<contactref element="C3" pad="P"/>
<contactref element="PWR_OUT" pad="3"/>
</signal>
<signal name="GND_5L">
<contactref element="C2" pad="N"/>
<contactref element="U6" pad="2"/>
<contactref element="U6" pad="GND"/>
<contactref element="C3" pad="N"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="VOUT_3_3">
<contactref element="RFBT_2" pad="2"/>
<contactref element="COUT_2" pad="1"/>
<contactref element="L1_3" pad="2"/>
<contactref element="PWR_OUT" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U5" pad="9"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="4"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="1"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="3"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="5"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="8"/>
<contactref element="R4" pad="1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
