<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="85.725" y1="0.635" x2="186.67" y2="0.635" width="0" layer="20"/>
<wire x1="186.67" y1="0.635" x2="186.67" y2="107.3025" width="0" layer="20"/>
<wire x1="186.67" y1="107.3025" x2="85.725" y2="107.3025" width="0" layer="20"/>
<wire x1="85.725" y1="107.3025" x2="85.725" y2="0.635" width="0" layer="20"/>
<text>JRO-JARS2.0-CLKDRV-1.0</text>
<text>Revision 1.0</text>
</plain>
<libraries>
<library name="jicamarca">
<packages>
<package name="MINIMELF">
<description>&lt;b&gt;Mini Melf Diode&lt;/b&gt;</description>
</package>
<package name="MSOP8">
</package>
<package name="PQFP52">
</package>
<package name="SOIC08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="OSC_SMD">
</package>
<package name="JICA_LOGO1">
</package>
<package name="BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
<package name="AK500/2">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
</package>
<package name="CT3528">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wuerth-elektronik">
<packages>
<package name="0805">
<description>Multilayer SMD</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="jicamarca" package="PQFP52" value="IC_CDC2586">
<attribute name="DIGIKEY#" value="296-6690-5-ND"/>
<attribute name="MANF" value="Texas Instruments"/>
<attribute name="MANF#" value="CDC2586PAH"/>
</element>
<element name="R1" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="L1" library="jicamarca" package="C1206" value="FER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="240-2415-1-ND"/>
<attribute name="MANF" value="Laird-Signal Integrity Products"/>
<attribute name="MANF#" value="HZ1206E601R-10"/>
</element>
<element name="R2" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R3" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R4" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R5" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R6" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R7" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R8" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R9" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R10" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R11" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R12" library="jicamarca" package="R0603" value="24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="24:MCR03ERTF24R0:RHM24CFCT-ND|25.5:MCR03ERTF25R5:RHM25.5CFCT-ND|49.9:MCR03ERTF49R9:RHM49.9CFCT-ND|178:MCR03ERTF1780:RHM178CFCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R14" library="jicamarca" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="L3" library="jicamarca" package="C1206" value="FER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="240-2415-1-ND"/>
<attribute name="MANF" value="Laird-Signal Integrity Products"/>
<attribute name="MANF#" value="HZ1206E601R-10"/>
</element>
<element name="X1" library="jicamarca" package="BU-SMA-V" value="CLK1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X2" library="jicamarca" package="BU-SMA-V" value="CLK2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X3" library="jicamarca" package="BU-SMA-V" value="CLK3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X4" library="jicamarca" package="BU-SMA-V" value="CLK4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X5" library="jicamarca" package="BU-SMA-V" value="CLK5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X6" library="jicamarca" package="BU-SMA-V" value="CLK6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X7" library="jicamarca" package="BU-SMA-V" value="CLK7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X8" library="jicamarca" package="BU-SMA-V" value="CLK8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X9" library="jicamarca" package="BU-SMA-V" value="CLK9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X10" library="jicamarca" package="BU-SMA-V" value="CLK10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X11" library="jicamarca" package="BU-SMA-V" value="CLK11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="X12" library="jicamarca" package="BU-SMA-V" value="CLK12">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="IC2" library="jicamarca" package="SOIC08" value="SW_SA630D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="568-1206-5-ND"/>
<attribute name="MANF" value="NXP"/>
<attribute name="MANF#" value="SA630D/01,112"/>
</element>
<element name="X13" library="jicamarca" package="BU-SMA-V" value="CLK_EXT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="WM5543-ND"/>
<attribute name="MANF" value="Molex Inc"/>
<attribute name="MANF#" value="0733910060"/>
</element>
<element name="R15" library="jicamarca" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R16" library="jicamarca" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="D1" library="jicamarca" package="MINIMELF" value="DIODE_BAT42SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="BAT42WS-FDITR-ND"/>
<attribute name="MANF" value="Diodes Incorporated"/>
<attribute name="MANF#" value="BAT42WS-7-F"/>
</element>
<element name="D2" library="jicamarca" package="MINIMELF" value="DIODE_BAT42SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="BAT42WS-FDITR-ND"/>
<attribute name="MANF" value="Diodes Incorporated"/>
<attribute name="MANF#" value="BAT42WS-7-F"/>
</element>
<element name="C2" library="jicamarca" package="C0805" value="0.01u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="OSC1" library="jicamarca" package="OSC_SMD" value="OSC_CW542CT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="CW542CT-ND"/>
<attribute name="MANF" value="Connor-Winfield"/>
<attribute name="MANF#" value="CWX813-060.0M"/>
</element>
<element name="C3" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C4" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="IC3" library="jicamarca" package="MSOP8" value="IC_MIC5219-3.3YMM">
<attribute name="NAME"/>
<attribute name="DIGIKEY#" value="576-1281-1-ND"/>
<attribute name="MANF" value="Micrel Inc"/>
<attribute name="MANF#" value="MIC5219-3.3YM5 TR"/>
</element>
<element name="C5" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C6" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C8" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C10" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C11" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C9" library="jicamarca" package="CT3528" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="2.2u:T491B225M020AT:399-8308-1-ND|4.7u:T491B475M020AT:399-8324-1-ND|10u:T491B106M020AT:399-8300-1-ND"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C7" library="jicamarca" package="CT3528" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="2.2u:T491B225M020AT:399-8308-1-ND|4.7u:T491B475M020AT:399-8324-1-ND|10u:T491B106M020AT:399-8300-1-ND"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C1" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="IC4" library="jicamarca" package="MSOP8" value="IC_MIC5219-3.3YMM">
<attribute name="NAME"/>
<attribute name="DSSAD" value="sdfdsfdsfdsf"/>
<attribute name="DIGIKEY#" value="576-1281-1-ND"/>
<attribute name="MANF" value="Micrel Inc"/>
<attribute name="MANF#" value="MIC5219-3.3YM5 TR"/>
</element>
<element name="C15" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C16" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C17" library="jicamarca" package="CT3528" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="2.2u:T491B225M020AT:399-8308-1-ND|4.7u:T491B475M020AT:399-8324-1-ND|10u:T491B106M020AT:399-8300-1-ND"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C19" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C20" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C21" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C22" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C23" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C24" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C25" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C26" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C27" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C28" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C29" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C30" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C31" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C32" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C33" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C34" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C35" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C36" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C37" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C38" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C39" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C40" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C49" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C50" library="jicamarca" package="C0805" value="0.01u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C51" library="jicamarca" package="C0805" value="0.01u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C52" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C53" library="jicamarca" package="CT3528" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="2.2u:T491B225M020AT:399-8308-1-ND|4.7u:T491B475M020AT:399-8324-1-ND|10u:T491B106M020AT:399-8300-1-ND"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R17" library="jicamarca" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="LED1" library="jicamarca" package="CHIPLED_0603" value="APT1608SGC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="APT1608SGC:APT1608SGC:754-1121-1-ND:Kingbright Company LLC"/>
<attribute name="MANF" value="OSRAM"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="R13" library="jicamarca" package="R0603" value="300">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C12" library="jicamarca" package="C0805" value="220p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C13" library="jicamarca" package="CT3528" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="2.2u:T491B225M020AT:399-8308-1-ND|4.7u:T491B475M020AT:399-8324-1-ND|10u:T491B106M020AT:399-8300-1-ND"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C14" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="C18" library="jicamarca" package="C0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="220p:CL21B221KBANFNC:1276-2473-1-ND|470p:CL21B471KBANNNC:1276-1300-1-ND|1000p:CL21B102KBANNNC:1276-1020-1-ND |0.1u:CL21B104KBCNNNC:1276-1003-1-ND|0.01u:CL21B103KBANNNC:1276-1015-1-ND|4.7u:CL21A475KBQNNNE:1276-1248-1-ND|10u:CL21A106KAFN3NE:1276-2890-1-ND"/>
<attribute name="MANF" value="Samsung"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="X14" library="jicamarca" package="AK500/2" value="POWER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY#" value="ED1623-ND"/>
<attribute name="MANF" value="On Shore Technology"/>
<attribute name="MANF#" value="ED500/2DS"/>
</element>
<element name="E$1" library="jicamarca" package="JICA_LOGO1" value=""/>
<element name="R18" library="jicamarca" package="R0603" value="10k">
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
</element>
<element name="JP1" library="jumper" package="JP1" value=""/>
<element name="L2" library="wuerth-elektronik" package="0805" value=""/>
<element name="R19" library="jicamarca" package="R0603" value="1k">
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="jicamarca" package="R0603" value="1k">
<attribute name="DIGIKEY#" value="USE_DIGIKEY#S"/>
<attribute name="DIGIKEY#S" value="0:MCR03ERTJ000:RHM0.0CGCT-ND|10:MCR03ERTJ100:RHM10CGCT-ND|27:MCR03ERTF27R0:RHM27CFCT-ND|68:MCR03ERTJ680:RHM68CGCT-ND|100:MCR03ERTJ101:RHM100CGCT-ND|220:MCR03ERTJ221:RHM220CGCT-ND|300:MCR03ERTJ301:RHM300CGCT-ND|330:MCR03ERTJ331:RHM330CGCT-ND|470:MCR03ERTJ471:RHM470CGCT-ND|1k:MCR03ERTJ102:RHM1.0KCGCT-ND|2k:MCR03ERTJ202:RHM2KCGCT-ND|2.2k:MCR03ERTJ222:RHM2.2KCGCT-ND|10k:MCR03ERTJ103:RHM10KCGCT-ND"/>
<attribute name="MANF" value="Rohm Semiconductor"/>
<attribute name="MANF#" value="USE_DIGIKEY#S"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP1" value=""/>
<element name="JP3" library="jumper" package="JP1" value=""/>
</elements>
<signals>
<signal name="PE">
<contactref element="IC1" pad="P1"/>
<contactref element="IC1" pad="P4"/>
<contactref element="IC1" pad="P7"/>
<contactref element="IC1" pad="P10"/>
<contactref element="IC1" pad="P11"/>
<contactref element="IC1" pad="P14"/>
<contactref element="IC1" pad="P17"/>
<contactref element="IC1" pad="P20"/>
<contactref element="IC1" pad="P21"/>
<contactref element="IC1" pad="P24"/>
<contactref element="IC1" pad="P27"/>
<contactref element="IC1" pad="P30"/>
<contactref element="IC1" pad="P31"/>
<contactref element="IC1" pad="P34"/>
<contactref element="IC1" pad="P37"/>
<contactref element="IC1" pad="P52"/>
<contactref element="R14" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="X1" pad="5"/>
<contactref element="X12" pad="4"/>
<contactref element="X12" pad="3"/>
<contactref element="X12" pad="5"/>
<contactref element="X11" pad="4"/>
<contactref element="X11" pad="3"/>
<contactref element="X11" pad="5"/>
<contactref element="X10" pad="4"/>
<contactref element="X10" pad="3"/>
<contactref element="X10" pad="5"/>
<contactref element="X9" pad="4"/>
<contactref element="X9" pad="3"/>
<contactref element="X9" pad="5"/>
<contactref element="X8" pad="4"/>
<contactref element="X8" pad="3"/>
<contactref element="X8" pad="5"/>
<contactref element="X7" pad="4"/>
<contactref element="X7" pad="3"/>
<contactref element="X7" pad="5"/>
<contactref element="X6" pad="4"/>
<contactref element="X6" pad="3"/>
<contactref element="X6" pad="5"/>
<contactref element="X5" pad="4"/>
<contactref element="X5" pad="3"/>
<contactref element="X5" pad="5"/>
<contactref element="X4" pad="4"/>
<contactref element="X4" pad="3"/>
<contactref element="X4" pad="5"/>
<contactref element="X3" pad="4"/>
<contactref element="X3" pad="3"/>
<contactref element="X3" pad="5"/>
<contactref element="X2" pad="4"/>
<contactref element="X2" pad="3"/>
<contactref element="X2" pad="5"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="2"/>
<contactref element="X3" pad="2"/>
<contactref element="X4" pad="2"/>
<contactref element="X5" pad="2"/>
<contactref element="X7" pad="2"/>
<contactref element="X6" pad="2"/>
<contactref element="X8" pad="2"/>
<contactref element="X9" pad="2"/>
<contactref element="X10" pad="2"/>
<contactref element="X11" pad="2"/>
<contactref element="X12" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="X13" pad="2"/>
<contactref element="X13" pad="5"/>
<contactref element="X13" pad="3"/>
<contactref element="X13" pad="4"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="7"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="OSC1" pad="2"/>
<contactref element="C9" pad="-"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="-"/>
<contactref element="C8" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C17" pad="-"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="5"/>
<contactref element="C19" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="-"/>
<contactref element="C14" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="X14" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="OCLK2_R">
<contactref element="IC1" pad="P5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="OCLK3_R">
<contactref element="IC1" pad="P8"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="OCLK4_R">
<contactref element="IC1" pad="P12"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="OCLK5_R">
<contactref element="IC1" pad="P15"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="OCLK6_R">
<contactref element="IC1" pad="P18"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="OCLK7_R">
<contactref element="IC1" pad="P22"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="OCLK8_R">
<contactref element="IC1" pad="P25"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="OCLK9_R">
<contactref element="IC1" pad="P28"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="OCLK10_R">
<contactref element="IC1" pad="P32"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="OCLK11_R">
<contactref element="IC1" pad="P35"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="OCLK12_R">
<contactref element="IC1" pad="P38"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="OCLK1">
<contactref element="R1" pad="2"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="OCLK2">
<contactref element="R2" pad="2"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="OCLK3">
<contactref element="R3" pad="2"/>
<contactref element="X3" pad="1"/>
</signal>
<signal name="OCLK4">
<contactref element="R4" pad="2"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="OCLK5">
<contactref element="R5" pad="2"/>
<contactref element="X5" pad="1"/>
</signal>
<signal name="OCLK6">
<contactref element="R6" pad="2"/>
<contactref element="X6" pad="1"/>
</signal>
<signal name="OCLK7">
<contactref element="R7" pad="2"/>
<contactref element="X7" pad="1"/>
</signal>
<signal name="OCLK8">
<contactref element="R8" pad="2"/>
<contactref element="X8" pad="1"/>
</signal>
<signal name="OCLK9">
<contactref element="R9" pad="2"/>
<contactref element="X9" pad="1"/>
</signal>
<signal name="OCLK10">
<contactref element="R10" pad="2"/>
<contactref element="X10" pad="1"/>
</signal>
<signal name="OCLK11">
<contactref element="R11" pad="2"/>
<contactref element="X11" pad="1"/>
</signal>
<signal name="OCLK12">
<contactref element="R12" pad="2"/>
<contactref element="X12" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="IC1" pad="P42"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R14" pad="2"/>
<contactref element="IC1" pad="P41"/>
</signal>
<signal name="SEL1">
<contactref element="IC1" pad="P51"/>
<contactref element="JP2" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="SEL0">
<contactref element="IC1" pad="P50"/>
<contactref element="R20" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="CLK_IN">
<contactref element="IC1" pad="P45"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="3.3VAC">
<contactref element="IC1" pad="P46"/>
<contactref element="IC1" pad="P43"/>
<contactref element="L3" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="C53" pad="+"/>
<contactref element="C52" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="C50" pad="1"/>
</signal>
<signal name="EXT_CLK">
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$46">
<contactref element="IC2" pad="7"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="X13" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="3.3VDC">
<contactref element="R15" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="P40"/>
<contactref element="IC1" pad="P3"/>
<contactref element="IC1" pad="P39"/>
<contactref element="IC1" pad="P36"/>
<contactref element="IC1" pad="P33"/>
<contactref element="IC1" pad="P29"/>
<contactref element="IC1" pad="P26"/>
<contactref element="IC1" pad="P23"/>
<contactref element="IC1" pad="P19"/>
<contactref element="IC1" pad="P16"/>
<contactref element="IC1" pad="P13"/>
<contactref element="IC1" pad="P9"/>
<contactref element="IC1" pad="P6"/>
<contactref element="L3" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="+"/>
<contactref element="C6" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="OUT_OSC">
<contactref element="OSC1" pad="3"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$48">
<contactref element="IC3" pad="4"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="V_INPUT">
<contactref element="IC3" pad="2"/>
<contactref element="C9" pad="+"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C17" pad="+"/>
<contactref element="R18" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="IC4" pad="4"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="3.3VDC_OSC">
<contactref element="IC4" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="OSC1" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="OSC1" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="+"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="IC1" pad="P47"/>
<contactref element="IC1" pad="P49"/>
<contactref element="L1" pad="1"/>
<contactref element="C49" pad="2"/>
<contactref element="C53" pad="-"/>
<contactref element="C52" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="C50" pad="2"/>
</signal>
<signal name="OCLK1_R">
<contactref element="IC1" pad="P48"/>
<contactref element="IC1" pad="P2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R18" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="V_SUPPLY">
<contactref element="L2" pad="1"/>
<contactref element="X14" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
